კონტროლერი

ძირითადი მოთხოვნა:

* საკომუნიკაცია პორტი: Wi-Fi
* ინტეგრაციის საშუალება: API, SDK

მწარმოებელი: huidu

მოდელი: Single-dual Color Controller HD-W63



|  |  |
| --- | --- |
| **Contents** | **Parameters** |
| Support module | Single Color/ Dual Color /Tricolor conventional scanning methods |
| Control range | Single color: 1024\*128Dual color: 512\*128 |
| FLASH Capacity | 4M Byte |
| Communication Port | U-Disk、Wi-Fi |
| Support Colorful | Full-color module can display red, green, blue, yellow, purple, green, white |
| Program Quantity | Max 1000pcs Programs. Can play by time section or control by buttons. |
| Area Quantity | 20 areas with separate zone, and separated special effects and border |
| Display Showing | Text、Picture、3DText、Animation（SWF）、Excel、Timing、Temperatures（humidity）、Count、Lunar calendar |
| Display | Sequence display, button switch, remote control |
|  Display effect  | 1、Text、Picture, Time, Timing 、Temperature or temperature and humidity (external module required) Display2、Support program border, regional border settings, custom borders3、A variety of action display4、More than 40 kinds of text effects display5、Support for simple animations word6、Support outline fonts, stroke fonts and other settings7、Support for regional text background settings8、Support Excel form directly adding |
| Clock function | 1、Support Digital Clock/ Dial Clock / Lunar Time/2、Countdown /Count up, Button Countdown / Count up3、The font、size、color and position can be set freely4、Support multiple time zones |
| Extended Equipment | Temperatures、Humidity、IR Remoter、Photosensitive sensors、etc. |
| Automatic switch screen | Support timer switch machine |
| Dimming | Support three brightness adjustment mode |