**ტენდერი: სს „სადაზღვევო კომპანია ალდაგის“ უწყვეტი კვების წყაროს (UPS) შესყიდვაზე**

**დანართი 1**

გთხოვთ მოგვწეროთ ქვევით მითითებული ინფორმაცია:

1. სატენდერო წინადადების ფასი უნდა იყოს წარმოდგენილი USD-ში. ერთეულის ფასი უნდა მოიცავდეს როგორც შესყიდვის ობიექტის მიწოდებასთან დაკავშირებულ ყველა ხარჯს თბილისის ფარგლებში, ასევე დ.ღ.გ-ს და საქართველოს კანონმდებლობით გათვალისწინებულ ყველა სხვა გადასახადს.
2. გთხოვთ ცალკე მიუთითოთ თანხის გადახდის პირობები
3. გარანტიაზე საქართველოში უნდა ემსახურებოდეს სერვის ცენტრი

**ლოტი 1**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Technical Specifications** | **რაოდენობა** | **გარანტია თვე** | **ერთეულის ფასი ლარი დღგ-ს ჩათვლით** | **შეკვედიდან მიწოდების ვადა (სამუშაო დღე)** |
| **Output**  Output power capacity  1.0 KWatts / 1.5 kVA  Max Configurable Power (Watts)  1.0 KWatts / 1.5 kVA  Nominal Output Voltage  230V  Output Voltage Note  Configurable for 220 : 230 or 240 nominal output voltage  Output Voltage Distortion  Less than 5% at full load  Output Frequency (sync to mains)  47 - 53 Hz for 50 Hz nominal, 57 - 63 Hz for 60 Hz nominal  Other Output Voltages  220, 240  Topology  Line Interactive  Output Connections  (4) IEC 320 C13 (Battery Backup)  (2) IEC Jumpers (Battery Backup)  Transfer Time  2ms typical  **Input**  Nominal Input Voltage 230V  Input frequency 50/60 Hz +/- 3 Hz (auto sensing)  Input Connections  IEC-320 C14  Input voltage range for main operations  160 - 286V  Input voltage adjustable range for mains operation  151 - 302V  Other Input Voltages  220, 240  **Physical**  Maximum Height  86mm, 8.6CM  Maximum Width  432mm, 43.2CM  Maximum Depth  457mm, 45.7CM  Maximum Rack Height 2U  **Batteries & Runtime**  Battery type - Maintenance-free sealed Lead-Acid battery with suspended electrolyte : leakproof  Typical recharge time - 3hour(s)  Expected Battery Life (years) - 4-6  RBC Quantity - 1  **Communications & Management**  Interface Port(s) RJ-45 Serial, SmartSlot, USB  Control panel  Multi-function LCD status and control console  Audible Alarm  Alarm when on battery : distinctive low battery alarm : configurable delays  Emergency Power Off (EPO)  Optional  Available SmartSlot™ Interface Quantity 1 | **2** | 3 years repair or replace (excluding battery) and 2 year for battery |  | **7** |

|  |
| --- |
|  |

**ლოტი 2**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Technical Specifications** | **რაოდენობა** | **გარანტია თვე** | **ერთეულის ფასი ლარი დღგ-ს ჩათვლით** | **შეკვედიდან მიწოდების ვადა (სამუშაო დღე)** |
| **Output**  Output power capacity 2.7 KWatts / 3.0 kVA  Max Configurable Power (Watts) 2.7 KWatts / 3.0 kVA  Nominal Output Voltage 230V  Output Voltage Note Configurable for 220 : 230 or 240 nominal output voltage  Output Frequency (sync to mains) 47 - 53 Hz for 50 Hz nominal, 57 - 63 Hz for 60 Hz nominal  Other Output Voltages 220, 240  Topology Line Interactive  Waveform type Sine wave  Output Connections (3) IEC Jumpers (Battery Backup)  (1) IEC 320 C19 (Battery Backup)  (8) IEC 320 C13 (Battery Backup)  Transfer Time  4ms typical : 8ms maximum  **Input**  Nominal Input Voltage 230V  Input frequency 50/60 Hz +/- 3 Hz (auto sensing)  Input Connections British BS1363A, IEC-320 C20, Schuko CEE 7/EU1-16P  Cord Length 2meters  Input voltage range for main operations 160 - 286V  Input voltage adjustable range for mains  operation 151 - 302V  Number of Power Cords 1  Other Input Voltages 220, 240  **Batteries & Runtime**  Battery type Maintenance-free sealed Lead-Acid battery with suspended electrolyte : leakproof  Typical recharge time 3hour(s)  Expected Battery Life (years) 3 - 5  RBC Quantity 1  **Communications & Management**  Interface Port(s) USB  Control panel LED status display with On Line : On Battery : Replace Battery and Overload indicators, Multi-  function LCD status and control console  Audible Alarm Alarm when on battery : distinctive low battery alarm : configurable delays  Available SmartSlotTM Interface Quantity 1  **Physical**  Maximum Height 86mm, 8.6CM  Maximum Width 480mm, 48.0CM  Maximum Depth 683mm, 68.3CM  Maximum Rack Height 2U | 1 | 3 years repair or replace (excluding battery) and 2 year for battery |  |  |